PANTHER XP12 Startup:

Fuel Levers (Overhead - Back)  | Off 
Engine Control Levers (Overhead - Back) | Off 
Battery  (Center Panel)  | On 
26V OK ? | Check
Electrical Parameters | Check
Strobe Light on
Landing and Taxi Lights (Upper Panel Landing Lights) | On
Inverter (Center Panel) | On 
Annunciator Test (Annunciator Panel) | Check
Release Rotor Brake (Center Panel) | Off (full forward)
Fuel Quantity | Check 
DC Generators (Center Panel DC Switch) | On 

Engine1 or 2
Fuel Lever | Open (Forward) 
Control Lever | Ground Idle first detent
To Start, Press (ctrl 1) Release at 50% Ng | Started
AC Generator (Center Panel AC Switch) | On
Inverter and Avionics on 

BEFORE TAKEOFF 
Navigation Lights | On
Engine 1 and 2, Fuel Levers open to max | Check open to max
Engine 1 and 2, Power Levers | Set Ng to 85 %
Rotor RPM 400 | Check
 
